ABS may shrink during printing, so it is sometimes necessary to resize the STL model, for example, by multiplying X, Y, and Z dimensions by 1.05. 
Sometimes you may have to proceed by trial and error.